This folder contains detail for Test_Case2.

Source IP        = 192.168.10.20, which is c0a8 0a14 in hex
Destination IP   = 192.168.10.10, which is c0a8 0a0a in hex
Source Port      = 2341, which is 0925 in hex,
Destination Port = 1200, which is 04B0 in hex.

For the SYN packet, the SYN Flag in the header has a value of 1.
For the SYN+ACK packet, the SYN and ACK flags in the header have a value of 1.
For the ACK packet, the ACK flag in the header has a value of 1.
For the FIN packet, the FIN flag in the header has a value of 1.
For the FIN+ACK packet, the FIN and ACK flags in the header have a value of 1.