This folder contains detail for Test_Case1.

Source IP        = 200.204.10.12, which is c8cc 0a0c in hex
Destination IP   = 200.204.10.14, which is c8cc 0a0e in hex
Source Port      = 1234, which is 04D2 in hex,
Destination Port = 4444, which is 115c in hex.

For the SYN packet, the SYN Flag in the header has a value of 1.
For the SYN+ACK packet, the SYN and ACK flags in the header have a value of 1.
For the ACK packet, the ACK flag in the header has a value of 1.
For the FIN packet, the FIN flag in the header has a value of 1.
For the FIN+ACK packet, the FIN and ACK flags in the header have a value of 1.